Shaun McCance
shaunm@gnome.org
Jim Campbell
jwcampbell@gmail.com
Michael Hill
mdhillca@gmail.com
Ekaterina Gerasimova
kittykat3756@gmail.com
L'identifiant unique attribué au périphérique réseau.
Luc Pionchon
pionchon.luc@gmail.com 2011
Claude Paroz
claude@2xlibre.net 2011
Alain Lojewski
allomervan@gmail.com 2011-2015
Julien Hardelin
jhardlin@orange.fr 2011, 2013
Bruno Brouard
annoa.b@gmail.com 2011-12
yanngnome
yannubuntu@gmail.com 2012
Nicolas Delvaux
contact@nicolas-delvaux.org 2012
Mickael Albertus
mickael.albertus@gmail.com 2012
Alexandre Franke
alexandre.franke@gmail.com 2015
Hydroxyp
hydroxyp@gmail.com 2020

# Adresse MAC

Une adresse MAC est un identifiant unique attribué à chaque périphérique réseau (comme une carte Wifi ou Ethernet) par le fabricant. MAC signifie Media Access Control et chaque identifiant est unique à chaque périphérique.

Une adresse MAC se compose de six groupes de deux caractères chacun, séparés par deux points. Voici un exemple d'adresse MAC : `00:1B:44:11:3A:B7`.

Pour identifier l'adresse MAC de votre périphérique réseau :

Open the Activities overview and start typing Network.

Cliquez sur Réseau pour ouvrir le panneau.

Choose which device, Wi-Fi or Wired, from the left pane.

The MAC address for the wired device will be displayed as the Hardware Address on the right.

Click the settings button to see the MAC address for the wireless device displayed as the Hardware Address in the Details panel.

In practice, you may need to modify or “spoof” a MAC address. For example, some internet service providers may require that a specific MAC address be used to access their service. If the network card stops working, and you need to swap a new card in, the service won’t work anymore. In such cases, you would need to spoof the MAC address.