Proxecto de documentación de GNOME
gnome-doc-list@gnome.org
Resolución de problemas en lectores de tarxetas multimedia.
Fran Diéguez
frandieguez@gnome.org 2011-2020

# Problemas no lector de tarxetas multimedia

Moitos computadores conteñen lectores para tarxetas de almacenamento SD, MMC, MS, CF e outras. Deberíanse detectar automaticamente e montar. Aquí pode ler algunha resolución de erro se non se detectan e montan automaticamente:

Asegúrese de que a tarxeta está inserida correctamente. Moitas tarxetas parecen que están ao revés cando se insiren correctamente. Asegúrese tamén de que a tarxeta está ben colocada na ranura; algunhas tarxetas, especialmente as CF requiren que se faga un pouco de forza para inserilas correctamente. (Teña coidado de non empurrar moi forte. Se choca contra algo sólido, non o force)

Open Files from the Activities overview. Does the inserted card appear in the left sidebar? Sometimes the card appears in this list but is not mounted; click it once to mount. (If the sidebar is not visible, press F9 or click Files in the top bar and select the Sidebar.)

If your card does not show up in the sidebar, press CtrlL, then type computer:/// and press Enter. If your card reader is correctly configured, the reader should come up as a drive when no card is present, and the card itself when the card has been mounted.

Se ve o lector de tarxetas pero non a tarxeta, o problema pode estar na tarxeta en si. Ténteo cunha tarxeta diferente ou probe a tarxeta nun lector de tarxetas se lles é posíbel.

If no cards or drives are shown when browsing the Computer location, it is possible that your card reader does not work with Linux due to driver issues. If your card reader is internal (inside the computer instead of sitting outside) this is more likely. The best solution is to directly connect your device (camera, cell phone, etc.) to a USB port on the computer. USB external card readers are also available, and are far better supported by Linux.