Shaun McCance
shaunm@gnome.org
Jim Campbell
jwcampbell@gmail.com
Michael Hill
mdhillca@gmail.com
Ekaterina Gerasimova
kittykat3756@gmail.com
Verkkolaittelle määritetty yksilöllinen tunniste.
Timo Jyrinki
timo.jyrinki@iki.fi 2012.
Jiri Grönroos
jiri.gronroos+l10n@iki.fi 2012-2020.

# Mikä MAC-osoite on?

MAC-osoite on yksilöllinen koodi, jonka valmistaja on määrittänyt tietylle verkkolaitteiden ryhmälle (kuten langattomalle verkkokortille tai Ethernet-kortille). MAC on lyhenne sanoista Media Access Control, ja jokainen koodi on laitekohtainen.

MAC-osoitteessa on kuusi kahden merkin sarjaa kaksoispisteellä eroteltuna (esimerkiksi `00:1B:44:11:3A:B7`).

Tietokoneen MAC-osoitteen selvittäminen:

Avaa Toiminnot-yleisnäkymä ja ala kirjoittamaan Verkko.

Napsauta Verkko.

Choose which device, Wi-Fi or Wired, from the left pane.

The MAC address for the wired device will be displayed as the Hardware Address on the right.

Click the settings button to see the MAC address for the wireless device displayed as the Hardware Address in the Details panel.

In practice, you may need to modify or “spoof” a MAC address. For example, some internet service providers may require that a specific MAC address be used to access their service. If the network card stops working, and you need to swap a new card in, the service won’t work anymore. In such cases, you would need to spoof the MAC address.