Dự án tài liệu GNOME
gnome-doc-list@gnome.org
Nếu bản in có vệt, mờ, thiếu màu, kiểm tra xem mực in còn không và đầu in có sạch không.
Nguyễn Thái Ngọc Duy
pclouds@gmail.com 2011-2012.

# Tại sao có vệt, mờ, thiếu màu khi in?

If your print-outs are streaky, faded, have lines on them that should not be there, or are otherwise poor in quality, this may be due to a problem with the printer or a low ink or toner supply.

# Chữ và ảnh mờ

You may be running out of ink or toner. Check your ink or toner supply and buy a new cartridge if necessary.

# Vệt và sọc

If you have an inkjet printer, the print head may be dirty or partially blocked. Try cleaning the print head. See the printer’s manual for instructions.

# Sai màu

The printer may have run out of one color of ink or toner. Check your ink or toner supply and buy a new cartridge if necessary.

# Jagged lines, or lines are not straight

If lines on your print-out that should be straight turn out jagged, you may need to align the print head. See the printer’s instruction manual for details on how to do this.