Jim Campbell
jcampbell@gnome.org
Πώς αφαιρείτε ένα κολλημένο χαρτί εξαρτάται από την κατασκευή και το μοντέλο του εκτυπωτή που έχετε.
Ελληνική μεταφραστική ομάδα GNOME
team@gnome.gr 2009-2016
Δημήτρης Σπίγγος
dmtrs32@gmail.com 2012-2015
Φώτης Τσάμης
ftsamis@gmail.com 2009
Μάριος Ζηντίλης
m.zindilis@dmajor.org 2009, 2010
Θάνος Τρυφωνίδης
tomtryf@gnome.org 2012-2016
Μαρία Μαυρίδου
mavridou@gmail.com 2014

# Αφαίρεση κολλημένου χαρτιού

Μερικές φορές οι εκτυπωτές τροφοδοτούν λαθεμένα φύλλα χαρτί και κολλάνε.

The manual for your printer will usually provide detailed instructions on how to clear paper jams. Usually, you will need to open one of the printer’s panels to find the jam inside and then firmly (but carefully!) pull the jammed paper out of the printer’s feeding mechanism.

Once the jam has been cleared you may need to press the printer’s resume button to start printing again. With some printers, you may even need to turn the printer off and then on again, and then start the print job again.